**HW – 3**

**Challenge 1**

1. Sample input is hard-coded for src\_pts\_nx2, dest\_pts\_nx2 and test\_pts\_nx2. User can select the inputs by using ginput as well. (Commented code is provided)
2. Similarly, provision for manually selecting the points is provided. (Commented code)
3. Warping works smoothly with two images only. For the third image, process runs without error. However, at some point Homography calculation messes up and the bounding box corners go awry.
4. Please find the results in MyPanorma folder.